KCT6-WCA V2.0 Upgrade Description

Hardware Version: V2.0

Software Version: V11.1.1.35

What’s New:

1. Modifying the configuration does not cause the image to stutter or blur.

2. Fixed other issues.

Notes:

1. This firmware only applies to KCT6-WCAV2.0. Check the product model before upgrading the firmware.

2. GUI Upgrade:

Unzip the downloaded file and save the upgrade file ending with **.bin** to the root directory of the USB storage device. Log in to the GUI of the NVR, navigate to **Configuration** > **Camera**, find the corresponding camera in the list of added cameras, and click the upgrade button on the right. You can also select multiple cameras and click the upgrade button to batch upgrade. Then unplug the mouse and insert the USB storage device into the USB port. After the upgrade file is detected, your camera will be upgraded automatically.

3. Web UI Upgrade:

Unzip the downloaded file. Log in to the web UI of the NVR, navigate to **Configuration** > **Camera**, locate the camera in the list of added cameras, click **Upgrade** on the far right, and select the file starting with **US\_** and ending with **.bin** to upgrade your camera.

4. Do not unplug the USB storage device or power off the device during the upgrade. Otherwise, the camera may be damaged.